**Indicative Critical Component List**

**Television (TV)**

| **Details of Critical Components used:** Model Name (Specify) : | | | | | |
| --- | --- | --- | --- | --- | --- |
| **Object / part No.** | **Manufacturer/ trademark** | **Type / model** | **Technical data** | **Standard** | **Mark(s) of conformity1)** |
| LCD Panel |  |  |  |  |  |
| Plastic Enclosure  (Back cover) |  |  |  |  |  |
| Cabinet |  |  |  |  |  |
| Pedestal Cover/Stand Material |  |  |  |  |  |
| Insulation sheet  (located between Power supply PCB and LCD panel chassis) |  |  |  |  |  |
| PCB Material  (Primary board) |  |  |  |  |  |
| PCB Material  (Secondary main board)  (if used) |  |  |  |  |  |
| Internal wire |  |  |  |  |  |
| LEDs,  If LASER Class applicable |  |  |  |  |  |
| ON/OFF Switch  (if used) |  |  |  |  |  |
| Power supply unit |  |  |  |  |  |
| **If power supply unit not certified:** | | | | | |
| Appliance Inlet  (if used) |  |  |  |  |  |
| Mains fuse |  |  |  |  |  |
| Bridging resistor in primary circuit  (if used) |  |  |  |  |  |
| Across the line capacitor / X capacitor |  |  |  |  |  |
| Line to chassis capacitor / Y capacitor |  |  |  |  |  |
| Opto-coupler |  |  |  |  |  |
| Inductor  (if used) |  |  |  |  |  |
| VDR / MOV  (if used) |  |  |  |  |  |
| Thermistor  (if used) |  |  |  |  |  |
| Transformer |  |  |  |  |  |
| Transformer’s Bobbin |  |  |  |  |  |
| Winding Wire |  |  |  |  |  |
| Triple insulated wire (TIW)  (if used) |  |  |  |  |  |
| Insulation Tape |  |  |  |  |  |
| Line filter coil  (if used) |  |  |  |  |  |
| Bobbin |  |  |  |  |  |
| **Power Cord Set:** | | | | | |
| Mains Plug |  |  |  |  |  |
| Cord |  |  |  |  |  |
| Appliance  Connector |  |  |  |  |  |

**Other required documents** -

1) Sample with proper marking label

2) Circuit Diagram

3) List of Safety Critical Components

4) Instruction & Service Manual

5) Transformer Details

6) Business License (Copy of Original + English Translated)

7) Trade Mark Certificate (Copy)

8) If Series inclusion then Declaration letter from the manufacturer